A (novel) Weakly-Compressible Volume-of-Fluid (VoF) Method for the Self Pressurisation of Cryogenic Storage Tanks

M.Y. Oomar\*1, A.G. Malan†1, L.C. Malan‡1, S. Zaleski§2, and F. Gambioli¶3

1 Industrial CFD Research Group, Department Mechanical Engineering, University of Cape Town, Private Bag X3, Rondebosch 7701, South Africa

2Department of Mechanical Engineering, Sorbonne Université and CNRS, Institut Jean Le Rond d’Alembert UMR 7190, F-75005 Paris, France

2Institut Universitaire de France, Paris, France

3 Airbus Operations Ltd Pegasus House, Aerospace Avenue, Filton, Bristol, BS43 7PA, England, U.K

April 13, 2023

The design of cryogenic storage tanks rely on accurate modelling of the self-pressurisation process which occurs due to heat transfer with the environment. This complex process involves gas compressibility, natural convection and phase change. In this context, an efficient and novel weakly-compressible Volume-of-Fluid (VoF) method is developed and implemented in ELEMEN- TAL® [1, 2, 3, 4]. The model is based on the two-fluid formulation proposed by Baer & Nun- ziato [5] and is reduced to a four-equation model via a non-dimensional analysis of a liquid-gas hydrogen system at saturation conditions. This is in the interest of reducing complexity and com- putational costs. The resulting model consists of a VoF transport equation, a gas phase continuity equation, and a one-fluid homogeneous momentum and thermal energy conservation method. The system of governing equations is solved using ELEMENTAL® ’s existing semi-implicit pressure- based projection method which is extended to include a simultaneous pressure and temperature solve. The developed model is then validated using standard test cases. These include an adiabatic syringe case to test the accuracy to model compressibility effects and a two-phase heat diffusion problem to validate non-isothermal effects. For all tested cases, a good correlation is obtained be- tween the numerical and analytical solution. Finally, to demonstrate the accuracy of the method for capturing liquid-gas hydrogen pressurisation, a 2D equivalent of the popular Flight-Weight case [6, 7] with a 50% liquid fill, is modelled. The modelled pressurisation shows a good correlation with experimental measurement.

\*omrmuh009@myuct.ac.za

†arnaud.malan@uct.ac.za

‡leon.malan@uct.ac.za

§stephane.zaleski@sorbonne-universite.fr

¶francesco.gambioli@airbus.com

**References**

1. J. Pattinson, A. G. Malan, and J. P. Meyer, “A cut-cell non-conforming cartesian mesh method for compressible and incompressible flow,” *International Journal for Numerical Methods in Engineering*, vol. 72, March 2008.
2. O. F. Oxtoby and A. G. Malan, “A matrix-free, implicit, incompressible fractional-step algo- rithm for fluid-structure interaction applications,” *Journal of Computational Physics*, vol. 231,

pp. 5389–5405, Jun 20 2012.

1. A. G. Malan and O. F. Oxtoby, “An accelerated, fully-coupled, parallel 3D hybrid finite- volume fluid-structure interaction scheme,” *Computer Methods in Applied Mechanics and Engineering*, vol. 253, pp. 426–438, Jan 1 2013.
2. J. A. Heyns, A. G. Malan, T. M. Harms, and O. F. Oxtoby, “A weakly compressible free- surface flow solver for liquid-gas systems using the volume-of-fluid approach,” *Journal of Computational Physics*, vol. 240, pp. 145–157, May 1 2013.
3. M. R. Baer and J. W. Nunziato, “A two-phase mixture theory for the Deflagaration - to - Detonation Transition ( DDT ) in reactive Granular Materials,” vol. 12, no. 6, pp. 861–889, 1986.
4. M. Hasan, C. S. Lin, and N. Vandresar, “Self-pressurization of a flightweight liquid hydro- gen storage tank subjected to low heat flux,” in *1991 ASME/AIChE National Heat Transfer Conference*, no. E-6095, 1991.
5. M. Kassemi and O. Kartuzova, “Effect of interfacial turbulence and accommodation coef- ficient on cfd predictions of pressurization and pressure control in cryogenic storage tank,” *Cryogenics*, vol. 74, pp. 138–153, 2016. 2015 Space Cryogenics Workshop, June 24–26, 2015, Phoenix, AZ Hosted by NASA Glenn Research Center, Cleveland, OH, USA.